Food Display Warmer

USER MANAUAL

Welcome to buy our products, all of us in this loyal employees expressed thanks to you! In order to give full play to the role of product performance, reduce unnecessary losses and injuries, the use of the product before you read the instruction manual and retain it for future reference.
Warning: Products must comply with instructions before use and, if violations of operation, an accident occurs, the factory will not be responsible.

1、Product safety ground before!
2、Rinse with water spray tube is strictly prohibited !
The new product design alone, beautiful shape, arc shape, adjustable three-tier display, surrounded by glass perspective, with optional thermostat with temperature display, make the temperature uniform, and with wet compensation, to keep food moisture.

Ⅰ、Performance

Thermostatic and Humidity

Ⅱ、Technical Parameters

	Item No
	Volts(V)
	Frequency
	Power( kW)
	Dimensions(mm)

	HW-1P
	220-240
	50-60Hz
	0.75
	350*430*500

	HW-1PA
	220-240
	50-60Hz
	0.5
	350*480*610

	HW-2P
	220-240
	50-60Hz
	0.8
	660*495*615

	HW-2PS
	220-240
	50-60Hz
	0.8
	660*495*615

	HW-3P
	220-240
	50-60Hz
	1.2
	950*495*615

	HW-3PS
	220-240
	50-60Hz
	1.2
	950*495*615

	HW-861
	220-240
	50-60Hz
	1.2
	350*455*580

	HW-862
	220-240
	50-60Hz
	1.3
	650*455*580

	HW-863
	220-240
	50-60Hz
	1.6
	900*455*580

	HW-60-1
	220-240
	50-60Hz
	1.84
	660*480*610

	HW-60-2
	220-240
	50-60Hz
	1.84
	900*480*610

	HW-60-3
	220-240
	50-60Hz
	2.2
	1200*480*610

	HW-580
	220-240
	50-60Hz
	1
	642*350*535

	HW-805
	220-240
	50-60Hz
	1.5
	865*360*625

	HW-815
	220-240
	50-60Hz
	0.65
	490*490*810

	HW-816
	220-240
	50-60Hz
	0.65
	490*490*810

	HW-500H
	220-240
	50-60Hz
	1.2
	380*420*760

	HW-500HA
	220-240
	50-60Hz
	1.2
	380*420*760

	HW-600H
	220-240
	50-60Hz
	1.6
	480*540*840

	HW-2X2
	220-240
	50-60Hz
	0.7
	700*655*740

	HW-2X3
	220-240
	50-60Hz
	1.4
	1100*655*740

	HW-2X4
	220-240
	50-60Hz
	1.4
	1200*655*740

	HW-6P-B
	220-240
	50-60Hz
	2.15
	1200*760*860

	HW-6P
	220-240
	50-60Hz
	2.2
	1500*760*860

	HW-6P-A
	220-240
	50-60Hz
	3.8
	1800*760*860

	HW-6P-C
	220-240
	50-60Hz
	4.8
	2200*760*860

	HW-1002
	220-240
	50-60Hz
	1.5
	610*440*700

	HW-1003
	220-240
	50-60Hz
	1.8
	880*440*700

	HW-1004
	220-240
	50-60Hz
	2.0
	1200*440*700


Ⅲ、Installs the operating procedure

1.Product safety ground before!
2. Product line voltage must be rated;
3. Each time before use is not connected to the power carried on the Sheng basin add water to 0.6 liters of water each time;
4. Power on, power indicator light, rotary heat switch, select the food holding temperature room temperature can rise, through natural flow, the temperature can be maintained the same levels;
5. In use, such as the need for lighting, lighting switch to open enable the operation more convenient and better display effect, at the same time open the top of the decorative lights, increase the display of results;
6. After use, clean the power supply must be cut off to prevent accidents;  

7. Use of the process, such as abnormal behavior, stop the role of troubleshooting to professionals, can continue to use.
8. This product does not apply to physical, sensory or mental deficiency or a lack of experience and knowledge of people (including children).
Water jet appliance part is strictly prohibited!

Ⅳ、Transport and Storage

During transport, prevent, vibration, impact, upside down, squeeze, waterproof, non-corrosive gas stored in the warehouse.   

Ⅴ、Cleaning and Maintenance

After use with non-corrosive cleaning agent, clean the cupboards bore.
2.Prohibited the use of paint has rubbed soluble liquid insulation cabinet surface!  

Ⅵ、Electrical schematic
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D1-Power Light     R-Heating Pipe       D2、D3-LED Lighting      D4、D5-Decorative lights    

WK-Thermostat     K1-Lighting switch   K2-Decorative light switch
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