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Food Warmer
Instruction manual

Model: INF-FW1
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Model:FW-1
    ★All stainless steel construction

     ★High-efficiency, easy to operate

     ★Durable and elegant design

     ★Must have someone to supervise when using 

     this product, to cut off the power when leaving
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Ⅰ. Introduction:
INF Series Food Warmer is made from high quality stainless steel which is stylish, durable and easy to clean. The warmer is equipped with highly reliable components so that they are energy-saving and safe. 

Ⅱ. Technical Specification:
	Model
	Voltage/frequency
	Input Power
	Dimension
	N.W.

	INF-FW1
	240V/50Hz
	0.3 kW
	340x565x500mm
	6kg


Ⅲ. Operating Instruction:
INF Series Food Warmer must be placed on a stable surface. 

Always use the food warmer in a well ventilated area.

Ⅳ.How to Use:
Place the machine on a safe and sturdy surface

After switching on the power the infrared element will start to heat up.

For safety turn the appliance off when not in use.

Ⅴ.  Note

Do please not to touch the infrared tube when in use.

Always use a professional technician for repairs.

Any repairs or maintenance must be carried out after the appliance is switched off.

If the appliance breaks down please do not disassemble yourself, contact your supplier for repair.

Packing list 
	Name
	Quantity
	Note

	Simple Food Warmer
	1
	

	Instruction book
	1
	


Ⅵ.Circuit Diagram
   ~240V/50Hz         
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SA1: ON / OFF Switch        HL: Heating Indication Light
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